**ISC Suspension N1 Coilover Installation for 08+ Lancer Evolution X**

**Rear:**

* Remove the carpet and other misc. covers from the trunk to access the tops of the rear strut mounts.



* Remove the 17mm Bolt that holds the strut in place to the lateral link



* Unbolt the top 14mm bolts
* Anti-Seize your new rear coilovers
* Install your coilovers and attach the top 14mm nuts in place if you have rear extenders you can route them as below.



* Re-install the bottom mount into the lateral link and tighten with the 17mm bolt.
* Adjust height as needed for what you’d like

**Front:**

* Remove the Wheel
* Remove the plastic bottom pieces from the base of the coilover that allows the ABS line to wrap around.



* Remove the ABS bracket held in place with a 12mm bolt
* Remove the two bottom 19mm Bolts that hold the base of the strut in place.



* Remove the three top 14mm Nuts that hold the nut in place.



* Anti-Seize your coilovers
* Install your coilovers and ensure the camber plate orientation is correct as shown



* Tighten the top 14mm bolts on top
* Anti-Seize all bolts
* Adjust height as needed